sys=CHECKLIST



devstack=Preflight

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=preflight checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,preflight checklist,-1.000000,

execute=1,Preflight checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Voice recorder?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

instring=preflight checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed in flight!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=VoiceRec,integer,,0.000000,,,,,,,,0,,

logic:

instring=set on

&&

[SYSTEMS.OVHDSIDER.VoiceRecorder]==[1.000000]

calc=[0.000000]

execute=2,ovhd-5,-1.000000,

execute=0,#On!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Oxygen?,0.000000,

execute=2,chkloxy,-1.000000,

logic:

instring=any

&&

[SYSTEMS.OVHDSIDER.VoiceRecorder]==[0.000000]

calc=[0.000000]

execute=2,ovhd-5,-1.000000,

execute=0,Not on; I will do!,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,voice-off,-1.000000,

execute=4,laminar/B738/toggle_switch/vcr_on,0.000000,

execute=2,voice-on,-1.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Oxygen?,0.000000,

execute=2,chkloxy,-1.000000,

logic:

calc=[0.000000]

out=Oxygen,integer,,0.000000,,,,,,,,0,,

logic:

instring=tested one hundred percent

||

instring=any

calc=[0.000000]

execute=2,chkloxy,-1.000000,

execute=1,Tested one hundred percent,0.000000,

execute=2,chklread,-1.000000,

execute=1,Navigation and display switches?,0.000000,

execute=2,chklovhddn,-1.000000,

logic:

calc=[0.000000]

out=DisplaySW0,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.VhfNavSource]>[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,vhf-nav,-1.000000,

execute=4,laminar/B738/toggle_switch/vhf_nav_source_lft,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklread,-1.000000,

logic:

[SYSTEMS.OVHDSIDEL.VhfNavSource]<[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,vhf-nav,-1.000000,

execute=4,laminar/B738/toggle_switch/vhf_nav_source_rgt,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklread,-1.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=DisplaySW1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.IrsSource]>[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,irs,-1.000000,

execute=4,laminar/B738/toggle_switch/irs_source_left,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

logic:

[SYSTEMS.OVHDSIDEL.IrsSource]<[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,irs,-1.000000,

execute=4,laminar/B738/toggle_switch/irs_source_right,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=DisplaySW2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.FmcSource]>[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,fmc,-1.000000,

execute=4,laminar/B738/toggle_switch/fmc_source_left,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

logic:

[SYSTEMS.OVHDSIDEL.FmcSource]<[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,fmc,-1.000000,

execute=4,laminar/B738/toggle_switch/fmc_source_right,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=DisplaySW3,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.SourceAuto]>[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,source,-1.000000,

execute=4,laminar/B738/toggle_switch/dspl_source_left,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

logic:

[SYSTEMS.OVHDSIDEL.SourceAuto]<[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,source,-1.000000,

execute=4,laminar/B738/toggle_switch/dspl_source_right,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=DisplaySW4,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.ControlSource]>[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,ctr-panel,-1.000000,

execute=4,laminar/B738/toggle_switch/dspl_ctrl_pnl_left,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

logic:

[SYSTEMS.OVHDSIDEL.ControlSource]<[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,ctr-panel,-1.000000,

execute=4,laminar/B738/toggle_switch/dspl_ctrl_pnl_right,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=DisplaySW,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.VhfNavSource]==[0.000000]

&&

[SYSTEMS.OVHDSIDEL.IrsSource]==[0.000000]

&&

[SYSTEMS.OVHDSIDEL.FmcSource]==[0.000000]

&&

[SYSTEMS.OVHDSIDEL.SourceAuto]==[0.000000]

&&

[SYSTEMS.OVHDSIDEL.ControlSource]==[0.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=12,preflight checklist,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Normal; auto!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Window heat?,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=WindowHeat1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WHeatLSide]!=[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,wh1-off,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_l_side,0.000000,

execute=2,wh1-on,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=WindowHeat2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WHeatLFwd]!=[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,wh2-off,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_l_fwd,0.000000,

execute=2,wh2-on,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=WindowHeat3,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WHeatRFwd]!=[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,wh3-off,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_r_fwd,0.000000,

execute=2,wh3-on,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=WindowHeat4,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WHeatRSide]!=[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,wh4-off,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_r_side,0.000000,

execute=2,wh4-on,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=WindowHeat,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WHeatLSide]==[1.000000]

&&

[SYSTEMS.OVHDSIDEL.WHeatLFwd]==[1.000000]

&&

[SYSTEMS.OVHDSIDEL.WHeatRSide]==[1.000000]

&&

[SYSTEMS.OVHDSIDEL.WHeatRFwd]==[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,On!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Pressurization mode selector,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=PressSel,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDER.PressModeSel]<=[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=1,Auto!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Flight instruments?,0.000000,

logic:

[SYSTEMS.OVHDSIDER.PressModeSel]==[2.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,altn-man,-1.000000,

execute=4,laminar/B738/toggle_switch/air_valve_ctrl_left,0.000000,

execute=2,altn-auto,0.000000,

execute=1,Auto!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Flight instruments?,0.000000,

logic:

[SYSTEMS.OVHDSIDER.PressModeSel]==[3.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,altn-man,-1.000000,

execute=4,laminar/B738/toggle_switch/air_valve_ctrl_left,0.000000,

execute=4,laminar/B738/toggle_switch/air_valve_ctrl_left,0.000000,

execute=2,altn-auto,0.000000,

execute=1,Auto!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Flight instruments?,0.000000,

logic:

calc=[0.000000]

out=FlightInstr,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.MCP.ChangeHPA_Cap]==[0.000000]

&&

[SYSTEMS.ELEC.BatterySW]==[1.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chklbarodn,-1.000000,

execute=4,laminar/B738/EFIS_control/fo/baro_in_hpa_dn,0.000000,

execute=8,jd/fo/needsetbaro,0.000000,

execute=8,jd/fo/needsetbaro1,0.000000,

execute=8,jd/fo/needsetbaro1,1.000000,

execute=2,chklbaroup,-1.000000,

execute=0,Heading <&SYSTEMS.POSITION.HDG_ND_Fo>,0.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Altitude <SYSTEMS.POSITION.AltimFO>,0.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Altimeter <&SYSTEMS.MCP.BaroSetInHgFo100>,0.000000,

execute=2,chklread,-1.000000,

execute=1,Parking brake?,0.000000,

logic:

instring=any

&&

[SYSTEMS.MCP.ChangeHPA_Cap]==[1.000000]

&&

[SYSTEMS.ELEC.BatterySW]==[1.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chklbarodn,-1.000000,

execute=4,laminar/B738/EFIS_control/fo/baro_in_hpa_up,0.000000,

execute=8,jd/fo/needsetbaro,0.000000,

execute=8,jd/fo/needsetbaro1,0.000000,

execute=8,jd/fo/needsetbaro1,1.000000,

execute=2,chklbaroup,-1.000000,

execute=0,Heading <&SYSTEMS.POSITION.HDG_ND_Fo>,0.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Altitude <SYSTEMS.POSITION.AltimFO>,0.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Altimeter <&SYSTEMS.MCP.BaroSetHpaFoFloor>,0.000000,

execute=2,chklread,-1.000000,

execute=1,Parking brake?,0.000000,

logic:

instring=any

&&

[SYSTEMS.ELEC.BatterySW]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Sir; we don't have power,0.000000,

execute=1,Preflight checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

instring=any

&&

instring=say the current course and altitude and baro

calc=[0.000000]

logic:

calc=[0.000000]

out=ParkingBrake,integer,,0.000000,,,,,,,,0,,

logic:

instring=set

&&

[SYSTEMS.BRAKES.ParkBrakeHandlePos]==[1.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=7,,0.300000,

execute=0,#Set!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Engine start levers?,0.000000,

logic:

instring=set

&&

[SYSTEMS.BRAKES.ParkBrakeHandlePos]==[0.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=7,,0.300000,

execute=1,Parking brake is not set,0.000000,

execute=2,chklread,-1.000000,

execute=1,Engine start levers?,0.000000,

logic:

calc=[0.000000]

out=EngStartLev,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.ENGINE.EngMastSumm]==[0.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=7,,0.300000,

execute=0,#Cutoff!,0.000000,

execute=2,chklread,-1.000000,

logic:

instring=any

&&

[SYSTEMS.ENGINE.EngMastSumm]>[0.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=1,Engine start levers not cutoff; Preflight checklist is not complete ,0.000000,

execute=3,,0.000000,

logic:

instring=cutoff

&&

[0.000000]==[1.000000]

calc=[0.000000]

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.CDU.CDUPreflight]==[0.000000]

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=12,preflight checklist,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Preflight checklist complete!,0.000000,

execute=2,look-front,-1.000000,

execute=0,Enter the missing data in the CDU,0.000000,

logic:

[SYSTEMS.CDU.CDUPreflight]==[1.000000]

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=12,preflight checklist,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Preflight checklist complete!,0.000000,

logic:

calc=[0.000000]



devstack=BeforeStart

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=before start checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,before start checklist,-1.000000,

execute=1,Before start checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Papers?,0.000000,

logic:

instring=before start checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed in flight!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Papers,integer,,0.000000,,,,,,,,0,,

logic:

instring=on board

||

instring=any

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=1,Flight deck door?,0.000000,

logic:

calc=[0.000000]

out=DeckDoor,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MISC.DeckDoor]>[0.000000]

calc=[0.000000]

execute=2,chkl-back,-1.000000,

execute=7,,0.200000,

execute=4,laminar/B738/toggle_switch/flt_dk_door_open,0.000000,

execute=7,,1.500000,

execute=2,chkl-ped,-1.000000,

execute=1,Closed and locked!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Fuel?,0.000000,

logic:

[SYSTEMS.MISC.DeckDoor]==[0.000000]

calc=[0.000000]

execute=2,chkl-back,-1.000000,

execute=7,,0.200000,

execute=2,chkl-ped,-1.000000,

execute=1,Closed and locked!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Fuel?,0.000000,

logic:

calc=[0.000000]

out=Fuel,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.MISC.TotalFuel]<[2500.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=1,Fuel quantity is too small for the flight. Before start checklist is not complete,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=3,,0.000000,

logic:

[0.000000]==[1.000000]

&&

instring=say fuel quantity

calc=[0.000000]

logic:

instring=any

&&

[SYSTEMS.MISC.TotalFuel]>[2500.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=1,#<SYSTEMS.MISC.TotalFuel> killogram on board!,0.000000,

execute=2,chklovhddn,-1.000000,

logic:

calc=[0.000000]

out=Pump1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LAftPumpSW]!=[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,aft-l-off,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft1,1.000000,

execute=2,aft-l-on,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pump2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]!=[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,fwd-l-off,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft2,1.000000,

execute=2,fwd-l-on,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pump3,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RFwdPumpSW]!=[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,fwd-r-off,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_rgt2,1.000000,

execute=2,fwd-r-on,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pump4,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RAftPumpSW]!=[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,aft-r-off,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_rgt1,1.000000,

execute=2,aft-r-on,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pump5,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.CenterTank]>[460.000000]

&&

[SYSTEMS.FUEL.LCtrPumpSW]!=[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,ctr-l-off,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr1,1.000000,

execute=2,ctr-l-on,0.000000,

logic:

[SYSTEMS.FUEL.CenterTank]<[460.000000]

&&

[SYSTEMS.FUEL.LCtrPumpSW]==[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,ctr-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr1,0.000000,

execute=2,ctr-l-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pump6,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.CenterTank]>[460.000000]

&&

[SYSTEMS.FUEL.RCtrPumpSW]!=[1.000000]

calc=[0.000000]

execute=2,ovhd-dn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,ctr-r-off,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr2,1.000000,

execute=2,ctr-r-on,0.000000,

logic:

[SYSTEMS.FUEL.CenterTank]<[460.000000]

&&

[SYSTEMS.FUEL.RCtrPumpSW]==[1.000000]

calc=[0.000000]

execute=2,ovhd-dn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,ctr-r-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr2,0.000000,

execute=2,ctr-r-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pumps,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.CenterTank]>[460.000000]

&&

[SYSTEMS.FUEL.PumpsAll]==[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,1.000000,

execute=1,Pumps on,0.000000,

execute=2,chklread,-1.000000,

execute=1,Passenger signs,0.000000,

logic:

[SYSTEMS.FUEL.CenterTank]<[460.000000]

&&

[SYSTEMS.FUEL.PumpsNoCtr]==[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,1.000000,

execute=1,Pumps on,0.000000,

execute=2,chklread,-1.000000,

execute=1,Passenger signs,0.000000,

logic:

calc=[0.000000]

out=Signs,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_SeatBeltsSW]==[0.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,belt-off,-1.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_dn,0.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_dn,0.000000,

execute=2,belt-on,0.000000,

execute=1,On!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Window?,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_SeatBeltsSW]==[1.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,belt-auto,-1.000000,

execute=4,laminar/B738/toggle_switch/seatbelt_sign_dn,0.000000,

execute=2,belt-on,0.000000,

execute=1,On!,0.000000,

execute=2,chklovhdup,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklread,-1.000000,

execute=1,Window?,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_SeatBeltsSW]==[2.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=1,On!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Window?,0.000000,

logic:

calc=[0.000000]

out=Windows,integer,,0.000000,,,,,,,,0,,

logic:

instring=locked

calc=[0.000000]

execute=2,chklwindow,-1.000000,

execute=1,locked,0.000000,

execute=2,chklread,-1.000000,

execute=1,M C P?,0.000000,

logic:

calc=[0.000000]

out=MCP1,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.FMS.V2]>[100.000000]

&&

[SYSTEMS.MCP.SpeedCompV2]!=[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=1,The M C P speed does not match the v2 speed from C D U,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=0,Before start checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

instring=any

&&

[SYSTEMS.FMS.V2]>[100.000000]

&&

[SYSTEMS.MCP.SpeedCompV2]==[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=1,Speed <&SYSTEMS.MCP.Speed>,0.000000,

logic:

instring=any

&&

[SYSTEMS.FMS.V2]<[100.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=1,V two is not set in m c d u,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=0,Before start checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

instring=Say speed, heading and altitude to MCP panel

&&

[1.000000]==[0.000000]

calc=[0.000000]

logic:

calc=[0.000000]

out=MCP2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MCP.ALT]<[1500.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=0,Heading <&SYSTEMS.MCP.HDG>,0.000000,

execute=0,Altitude <SYSTEMS.MCP.ALT>,0.000000,

execute=0,The altitude is too low for flight,0.000000,

execute=2,chklread,-1.000000,

execute=1,Takeoff speeds?,0.000000,

logic:

[SYSTEMS.MCP.ALT]>[1500.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=0,Heading <&SYSTEMS.MCP.HDG>,0.000000,

execute=0,Altitude <SYSTEMS.MCP.ALT>,0.000000,

execute=2,chklread,-1.000000,

execute=1,Takeoff speeds?,0.000000,

logic:

calc=[0.000000]

out=TakeoffSpeeds,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.FMS.SpeedsSum]<[300.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=2,chcduinit,-1.000000,

execute=4,laminar/B738/button/fmc2_init_ref,0.000000,

execute=2,chcdul6,-1.000000,

execute=4,laminar/B738/button/fmc2_6L,0.000000,

execute=2,chcdul1,-1.000000,

execute=4,laminar/B738/button/fmc2_1L,0.000000,

execute=2,chcdur6,-1.000000,

execute=4,laminar/B738/button/fmc2_6R,0.000000,

execute=4,laminar/B738/button/fmc2_6R,0.000000,

execute=4,laminar/B738/button/fmc2_6R,0.000000,

execute=4,laminar/B738/button/fmc2_6R,0.000000,

execute=4,laminar/B738/button/fmc2_6R,0.000000,

execute=2,chkl-cdu,-1.000000,

execute=1,Takeoff speeds is not set,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=0,Before start checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

instring=any

&&

[SYSTEMS.FMS.SpeedsSum]>[300.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=2,chcduinit,-1.000000,

execute=4,laminar/B738/button/fmc2_init_ref,0.000000,

execute=2,chcdul6,-1.000000,

execute=4,laminar/B738/button/fmc2_6L,0.000000,

execute=2,chcdul1,-1.000000,

execute=4,laminar/B738/button/fmc2_1L,0.000000,

execute=2,chcdur6,-1.000000,

execute=4,laminar/B738/button/fmc2_6R,0.000000,

execute=4,laminar/B738/button/fmc2_6R,0.000000,

execute=4,laminar/B738/button/fmc2_6R,0.000000,

execute=4,laminar/B738/button/fmc2_6R,0.000000,

execute=4,laminar/B738/button/fmc2_6R,0.000000,

execute=2,chkl-cdu,-1.000000,

execute=1,V one <SYSTEMS.FMS.V1>,0.000000,

execute=1,V rotate <SYSTEMS.FMS.VR>,0.000000,

execute=1,V two <SYSTEMS.FMS.V2>,0.000000,

execute=2,legs,-1.000000,

execute=4,laminar/B738/button/fmc2_legs,0.000000,

execute=2,chklread,-1.000000,

execute=1,CDU preflight?,0.000000,

logic:

instring=say takeoff speeds in cdu

&&

[1.000000]==[0.000000]

calc=[0.000000]

logic:

calc=[0.000000]

out=CDUPref,integer,,0.000000,,,,,,,,0,,

logic:

instring=complete

&&

[SYSTEMS.CDU.CDUPreflight]==[1.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=1,Complete,0.000000,

execute=2,chklread,-1.000000,

execute=1,Rudder and aileron trim?,0.000000,

logic:

instring=complete

&&

[SYSTEMS.CDU.CDUPreflight]==[0.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=1,CDU preflight is not complete,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=0,Before start checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=RudderTrim,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.PEDESTAL.RudderTrimComp]==[0.000000]

&&

[SYSTEMS.PEDESTAL.AileronTrimComp]==[0.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=0,#Free and zero!,0.000000,

execute=7,,1.000000,

execute=2,chklread,-1.000000,

execute=1,Taxi and takeoff briefing?,0.000000,

logic:

instring=any

&&

[SYSTEMS.PEDESTAL.RudderTrimComp]==[1.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=1,Rudder trim is not zero position,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Before checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

instring=free and zero

&&

[1.000000]==[0.000000]

calc=[0.000000]

logic:

instring=any

&&

[SYSTEMS.PEDESTAL.AileronTrimComp]==[1.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=1,Rudder trim is not zero position,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Before checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=TaxiBriefing,integer,,0.000000,,,,,,,,0,,

logic:

instring=complete

calc=[0.000000]

execute=0,#Complete!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Anti collision light?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

calc=[0.000000]

out=AntiCollision,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_BeaconSW]==[1.000000]

calc=[0.000000]

execute=2,chovhdrtdn,-1.000000,

execute=1,On,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_BeaconSW]==[0.000000]

calc=[0.000000]

execute=2,chovhdrtdn,-1.000000,

execute=2,beacon-off,-1.000000,

execute=8,sim/cockpit/electrical/beacon_lights_on,1.000000,

execute=2,beacon-on,0.000000,

execute=1,on,0.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=12,before start checklist,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Before start checklist complete,0.000000,

logic:

calc=[0.000000]



devstack=BeforeTaxi

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=before taxi checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,before taxi checklist,-1.000000,

execute=1,Before taxi checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Generators?,0.000000,

execute=2,chklovhddn,-1.000000,

logic:

instring=before taxi checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed in flight!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Generator1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.GenON]==[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,gen1-ctrl,-1.000000,

execute=4,laminar/B738/toggle_switch/gen1_dn,0.000000,

execute=2,gen1-on,0.000000,

execute=2,ovhd-dn,-1.000000,

logic:

[SYSTEMS.ELEC.GenON]==[3.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,gen1-ctrl,-1.000000,

execute=4,laminar/B738/toggle_switch/gen1_dn,0.000000,

execute=2,gen1-on,0.000000,

execute=2,ovhd-dn,-1.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Generator2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.GenON]==[2.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,gen2-ctrl,-1.000000,

execute=4,laminar/B738/toggle_switch/gen2_dn,0.000000,

execute=2,gen2-on,0.000000,

execute=2,ovhd-dn,-1.000000,

logic:

[SYSTEMS.ELEC.GenON]==[3.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,gen2-ctrl,-1.000000,

execute=4,laminar/B738/toggle_switch/gen2_dn,0.000000,

execute=2,gen2-on,0.000000,

execute=2,ovhd-dn,-1.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Generators,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.GenON]==[0.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,On,0.000000,

execute=2,chklread,-1.000000,

execute=1,Probe heat?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

[SYSTEMS.ELEC.GenON]!=[0.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Sir; we have a problem with the electrical system,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Before taxi checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

[SYSTEMS.ELEC.GenON]!=[0.000000]

&&

[SYSTEMS.ENGINE.Eng1N1]<[19.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Engine is not runing,0.000000,

execute=1,Before taxi checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

[SYSTEMS.ELEC.GenON]!=[0.000000]

&&

[SYSTEMS.ENGINE.Eng2N1]<[19.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Engine is not runing,0.000000,

execute=1,Before taxi checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=ProbeHeatA,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ProbeHeatA]==[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,probeaoff,-1.000000,

execute=8,laminar/B738/toggle_switch/capt_probes_pos,1.000000,

execute=2,probeaon,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=ProbeHeatB,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ProbeHeatB]==[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,probeboff,-1.000000,

execute=8,laminar/B738/toggle_switch/fo_probes_pos,1.000000,

execute=2,probebon,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=ProbeHeat,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ProbeHeatA]==[1.000000]

&&

[SYSTEMS.ICE.ProbeHeatB]==[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,On,0.000000,

execute=2,chklread,-1.000000,

execute=1,Anti ice?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

calc=[0.000000]

out=WingAntiIce,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.WingPB]>[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=1,Wing anti ice on,0.000000,

logic:

[SYSTEMS.ICE.WingPB]==[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=1,Wing anti ice off,0.000000,

logic:

calc=[0.000000]

out=EngAntiIce,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ENG1IcePB]==[1.000000]

&&

[SYSTEMS.ICE.ENG2IcePB]==[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=1,Engine one anti ice on,0.000000,

execute=2,chklread,-1.000000,

execute=1,Isolation valve?,0.000000,

logic:

[SYSTEMS.ICE.ENG1IcePB]==[0.000000]

&&

[SYSTEMS.ICE.ENG2IcePB]==[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=1,Engine two anti ice on,0.000000,

execute=2,chklread,-1.000000,

execute=1,Isolation valve?,0.000000,

logic:

[SYSTEMS.ICE.ENG1IcePB]==[0.000000]

&&

[SYSTEMS.ICE.ENG2IcePB]==[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=1,Engine anti ice off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Isolation valve?,0.000000,

logic:

[SYSTEMS.ICE.ENG1IcePB]==[1.000000]

&&

[SYSTEMS.ICE.ENG2IcePB]==[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=1,Engine anti ice on,0.000000,

execute=2,chklread,-1.000000,

execute=1,Isolation valve?,0.000000,

logic:

calc=[0.000000]

out=IsolValve,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.IsolValve]==[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,isol-v-off,-1.000000,

execute=8,laminar/B738/air/isolation_valve_pos,1.000000,

execute=2,isol-v-aut,0.000000,

execute=1,Auto,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklread,-1.000000,

execute=1,Engine start switches?,0.000000,

logic:

[SYSTEMS.AIR.IsolValve]==[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=1,Auto,0.000000,

execute=2,chklread,-1.000000,

execute=1,Engine start switches?,0.000000,

logic:

[SYSTEMS.AIR.IsolValve]==[2.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,isol-v-ope,-1.000000,

execute=8,laminar/B738/air/isolation_valve_pos,1.000000,

execute=2,isol-v-aut,0.000000,

execute=1,Auto,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklread,-1.000000,

execute=1,Engine start switches?,0.000000,

logic:

calc=[0.000000]

out=Eng1StartSw,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng1StartSW]!=[2.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,start1auto,-1.000000,

execute=4,laminar/B738/knob/eng1_start_right,0.000000,

execute=2,start1cont,0.000000,

execute=2,ovhd-dn,-1.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Eng2StartSw,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng2StartSW]!=[2.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,start2auto,-1.000000,

execute=4,laminar/B738/knob/eng2_start_right,0.000000,

execute=2,start2cont,0.000000,

execute=2,ovhd-dn,-1.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=EngStartSw,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng1StartSW]==[2.000000]

&&

[SYSTEMS.ENGINE.Eng2StartSW]==[2.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Continuous,0.000000,

execute=2,chklread,-1.000000,

execute=1,Recall?,0.000000,

logic:

calc=[0.000000]

out=Recall,integer,,0.000000,,,,,,,,0,,

logic:

instring=checked

&&

[SYSTEMS.MCP.MasterCaution]==[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Checked,0.000000,

execute=2,chklread,-1.000000,

execute=1,Autobrake?,0.000000,

logic:

instring=checked

&&

[SYSTEMS.MCP.MasterCaution]!=[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Sir; master caution illuminate,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Before taxi checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=AutoBrake,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.BRAKES.AutoBrakeSW]!=[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,brake-off,-1.000000,

execute=4,laminar/B738/knob/autobrake_dn,0.000000,

execute=4,laminar/B738/knob/autobrake_dn,0.000000,

execute=4,laminar/B738/knob/autobrake_dn,0.000000,

execute=4,laminar/B738/knob/autobrake_dn,0.000000,

execute=4,laminar/B738/knob/autobrake_dn,0.000000,

execute=2,brake-rto,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Rejected takeoff,0.000000,

execute=2,chklread,-1.000000,

execute=1,Engine start levers?,0.000000,

logic:

[SYSTEMS.BRAKES.AutoBrakeSW]==[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=1,Rejected takeoff,0.000000,

execute=2,chklread,-1.000000,

execute=1,Engine start levers?,0.000000,

logic:

calc=[0.000000]

out=EngStartLevers,integer,,0.000000,,,,,,,,0,,

logic:

instring=idle detent

&&

[SYSTEMS.ENGINE.EngMastSumm]!=[2.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=1,Sir; is not idle position,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Before taxi checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

instring=idle detent

&&

[SYSTEMS.ENGINE.EngMastSumm]==[2.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=1,#Idle detent!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Flight control,0.000000,

logic:

calc=[0.000000]

out=FlightControl,integer,,0.000000,,,,,,,,0,,

logic:

instring=checked

&&

[SYSTEMS.FLGHTCONT.FlightContrChecked]==[1.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=1,Checked,0.000000,

execute=2,chklread,-1.000000,

execute=1,Flaps?,0.000000,

logic:

instring=checked

&&

[SYSTEMS.FLGHTCONT.FlightContrChecked]==[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=1,Flight controls is not checked,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Before taxi checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Flaps,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.FLAPS.FlapsMove]==[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-ped,-1.000000,

execute=1,Flaps is not set,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Before taxi checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

instring=any

&&

[SYSTEMS.FLAPS.FlapCompCDU]!=[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-ped,-1.000000,

execute=1,Flaps are not set for takeoff position,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Before taxi checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

instring=any

&&

[SYSTEMS.FLAPS.FlapCompCDU]==[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-ped,-1.000000,

logic:

instring=say flap position

&&

[0.000000]==[1.000000]

calc=[0.000000]

logic:

instring=any

&&

[SYSTEMS.FLAPS.FlapsMove]>[0.750000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-ped,-1.000000,

execute=1,This position of the flaps is not used for takeoff,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Before taxi checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=FlapsSet,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FLAPS.FlapsMove]==[0.125000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Flaps one set; green light; detent,0.000000,

execute=2,chklread,-1.000000,

execute=1,Ground equipment?,0.000000,

logic:

[SYSTEMS.FLAPS.FlapsMove]==[0.250000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Flaps two set; green light; detent,0.000000,

execute=2,chklread,-1.000000,

execute=1,Ground equipment?,0.000000,

logic:

[SYSTEMS.FLAPS.FlapsMove]==[0.375000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Flaps five set; green light; detent,0.000000,

execute=2,chklread,-1.000000,

execute=1,Ground equipment?,0.000000,

logic:

[SYSTEMS.FLAPS.FlapsMove]==[0.500000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Flaps ten set; green light; detent,0.000000,

execute=2,chklread,-1.000000,

execute=1,Ground equipment?,0.000000,

logic:

[SYSTEMS.FLAPS.FlapsMove]==[0.625000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Flaps fifteen set; green light; detent,0.000000,

execute=2,chklread,-1.000000,

execute=1,Ground equipment?,0.000000,

logic:

[SYSTEMS.FLAPS.FlapsMove]==[0.750000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Flaps twenty five set; green light; detent,0.000000,

execute=2,chklread,-1.000000,

execute=1,Ground equipment?,0.000000,

logic:

calc=[0.000000]

out=Ground equipment,integer,,0.000000,,,,,,,,0,,

logic:

instring=clear

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=2,chklwindow,-1.000000,

execute=1,Clear,0.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=12,before taxi checklist,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Before taxi checklist complete,0.000000,

execute=2,rest01,-1.000000,

execute=0,Ready for Taxi!,0.000000,

logic:

calc=[0.000000]



devstack=BeforeTakeoff

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=before takeoff checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,before takeoff checklist,-1.000000,

execute=1,Before takeoff checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Flaps?,0.000000,

execute=2,chkl-mcp,-1.000000,

logic:

instring=before takeoff checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed in flight!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Flaps,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.FLAPS.FlapsMove]==[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-ped,-1.000000,

execute=1,Flaps are not set,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Before takeoff checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

instring=any

&&

[SYSTEMS.FLAPS.FlapCompCDU]!=[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-ped,-1.000000,

execute=1,Flaps is not set for takeoff position,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Before takeoff checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

instring=any

&&

[SYSTEMS.FLAPS.FlapCompCDU]==[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-ped,-1.000000,

logic:

instring=say flap position

&&

[0.000000]==[1.000000]

calc=[0.000000]

logic:

instring=any

&&

[SYSTEMS.FLAPS.FlapsMove]>[0.750000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-ped,-1.000000,

execute=1,This position of the flaps is not used for takeoff,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Before takeoff checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=FlapsSet,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FLAPS.FlapsMove]==[0.125000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Flaps one set; green light; detent,0.000000,

execute=2,chklread,-1.000000,

execute=1,Stabilizer trim?,0.000000,

logic:

[SYSTEMS.FLAPS.FlapsMove]==[0.250000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Flaps two set; green light; detent,0.000000,

execute=2,chklread,-1.000000,

execute=1,Stabilizer trim?,0.000000,

logic:

[SYSTEMS.FLAPS.FlapsMove]==[0.375000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Flaps five set; green light; detent,0.000000,

execute=2,chklread,-1.000000,

execute=1,Stabilizer trim?,0.000000,

logic:

[SYSTEMS.FLAPS.FlapsMove]==[0.500000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Flaps ten set; green light; detent,0.000000,

execute=2,chklread,-1.000000,

execute=1,Stabilizer trim?,0.000000,

logic:

[SYSTEMS.FLAPS.FlapsMove]==[0.625000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Flaps fifteen set; green light; detent,0.000000,

execute=2,chklread,-1.000000,

execute=1,Stabilizer trim?,0.000000,

logic:

[SYSTEMS.FLAPS.FlapsMove]==[0.750000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Flaps twenty five set; green light; detent,0.000000,

execute=2,chklread,-1.000000,

execute=1,Stabilizer trim?,0.000000,

logic:

calc=[0.000000]

out=StabTrim,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.THS.ThsError]<[0.250000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=1,<&SYSTEMS.THS.ThsToNeed10> units set,0.000000,

execute=2,chklread,-1.000000,

execute=1,Transponder?,0.000000,

logic:

[SYSTEMS.THS.ThsError]>[0.250000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=1,Is not set for takeoff position,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Before takoff checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Transponder,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.PEDESTAL.Transponder]!=[5.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,tcas-test,-1.000000,

execute=4,laminar/B738/knob/transponder_tara,0.000000,

execute=2,tcas-tara,-1.000000,

execute=2,chkl-ped,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,T A R A set,0.000000,

logic:

[SYSTEMS.PEDESTAL.Transponder]==[5.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=1,T A R A set,0.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=12,before takeoff checklist,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Before takeoff checklist complete,0.000000,

logic:

calc=[0.000000]



devstack=AfterTakeoffDL

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=after takeoff checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,after takeoff checklist,-1.000000,

execute=1,After takeoff checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Engine bleeds?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

instring=after takeoff checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed on the ground!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Eng1Bleeds,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Eng1BleedSW]!=[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,bleed1-off,-1.000000,

execute=8,laminar/B738/toggle_switch/bleed_air_1_pos,1.000000,

execute=2,bleed1-on,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Eng2Bleeds,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Eng2BleedSW]!=[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,bleed2-off,-1.000000,

execute=8,laminar/B738/toggle_switch/bleed_air_2_pos,1.000000,

execute=2,bleed2-on,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=EngineBleeds,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Eng1BleedSW]==[1.000000]

&&

[SYSTEMS.AIR.Eng2BleedSW]==[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,On,0.000000,

execute=2,chklread,-1.000000,

execute=1,Packs?,0.000000,

logic:

calc=[0.000000]

out=Pack1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Pack1]==[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,pack-1-off,-1.000000,

execute=8,laminar/B738/air/l_pack_pos,1.000000,

execute=2,pack-1-aut,0.000000,

logic:

[SYSTEMS.AIR.Pack1]==[2.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,pack-1-hig,-1.000000,

execute=8,laminar/B738/air/l_pack_pos,1.000000,

execute=2,pack-1-aut,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pack2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Pack2]==[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,pack-2-off,-1.000000,

execute=8,laminar/B738/air/r_pack_pos,1.000000,

execute=2,pack-2-aut,0.000000,

logic:

[SYSTEMS.AIR.Pack2]==[2.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,pack-2-hig,-1.000000,

execute=8,laminar/B738/air/r_pack_pos,1.000000,

execute=2,pack-2-aut,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Packs,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Pack1]==[1.000000]

&&

[SYSTEMS.AIR.Pack2]==[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Auto,0.000000,

execute=2,chklread,-1.000000,

execute=1,Landing gear?,0.000000,

logic:

calc=[0.000000]

out=LandingGear,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LG.LG_Lever]==[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,lg-up,-1.000000,

execute=8,laminar/B738/controls/gear_handle_down,0.500000,

execute=2,lg-off,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chkl-cdu,-1.000000,

execute=1,Up and Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Flaps?,0.000000,

logic:

[SYSTEMS.LG.LG_Lever]==[0.500000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=1,Up and off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Flaps?,0.000000,

logic:

[SYSTEMS.LG.LG_Lever]==[1.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=1,Down; After takeoff checklist is not complete,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Flaps,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FLAPS.FlapsMove]==[0.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Up; no light; detent,0.000000,

logic:

[SYSTEMS.FLAPS.FlapsMove]>[0.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Flaps extended,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,After takeoff checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=ToTheLine,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MCP.BaroStdCap]==[1.000000]

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=1,Altimeters?,0.000000,

logic:

[SYSTEMS.MCP.BaroStdCap]==[0.000000]

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=0,After takeoff checklist down to the line complete!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Altimeters,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MCP.BaroStdCap]==[1.000000]

&&

instring=any

&&

[SYSTEMS.MCP.BaroStdFo]==[0.000000]

calc=[0.000000]

execute=2,chbarostd,-1.000000,

execute=4,laminar/B738/EFIS_control/fo/push_button/std_press,0.000000,

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Standard set; cross checked,0.000000,

logic:

[SYSTEMS.MCP.BaroStdCap]==[1.000000]

&&

instring=any

&&

[SYSTEMS.MCP.BaroStdFo]==[1.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Standard set; cross checked,0.000000,

logic:

instring=say the baro set on the altimeter

&&

[1.000000]==[0.000000]

calc=[0.000000]

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[1.000000]

execute=2,chklread,-1.000000,

execute=12,after takeoff checklist,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,After takeoff checklist complete,0.000000,

logic:

calc=[0.000000]



devstack=AfterTakeoffBL

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=after takeoff checklist below the line

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,after takeoff checklist below the line,-1.000000,

execute=0,after takeoff checklist below the line!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Altimeters?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

instring=after takeoff checklist below the line

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed on the ground!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Altimeters,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MCP.BaroStdCap]==[1.000000]

&&

instring=any

&&

[SYSTEMS.MCP.BaroStdFo]==[0.000000]

calc=[0.000000]

execute=2,chbarostd,-1.000000,

execute=4,laminar/B738/EFIS_control/fo/push_button/std_press,0.000000,

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Standard set; cross checked,0.000000,

logic:

[SYSTEMS.MCP.BaroStdCap]==[1.000000]

&&

instring=any

&&

[SYSTEMS.MCP.BaroStdFo]==[1.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Standard set; cross checked,0.000000,

logic:

instring=say the baro set on the altimeter

&&

[1.000000]==[0.000000]

calc=[0.000000]

logic:

[SYSTEMS.MCP.BaroStdCap]==[0.000000]

&&

[0.000000]==[0.000000]

calc=[0.000000]

logic:

[SYSTEMS.MCP.BaroStdCap]==[0.000000]

&&

instring=any

&&

[SYSTEMS.MCP.BaroStdFo]==[1.000000]

calc=[0.000000]

execute=2,chbarostd,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Standard set; not cross checked,0.000000,

execute=0,Please check baro on Your side!,0.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[1.000000]

execute=2,chklread,-1.000000,

execute=12,after takeoff checklist below the line,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=0,After takeoff checklist below the line complete!,0.000000,

logic:

calc=[0.000000]



devstack=Descent

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=descent checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,descent checklist,-1.000000,

execute=1,Descent checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklovhdrt,-1.000000,

execute=1,Pressurization?,0.000000,

logic:

instring=descent checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed on the ground!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Press,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.FMS.AltDestMod]>[50.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=1,Landing altitude not set for landing,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Descent checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

instring=any

&&

[SYSTEMS.FMS.AltDestMod]<=[50.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=1,#Landing altitude <SYSTEMS.CABPRESS.LandAlt> set!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Recall?,0.000000,

logic:

instring=say landing altitude

&&

[0.000000]==[1.000000]

calc=[0.000000]

logic:

calc=[0.000000]

out=Recall,integer,,0.000000,,,,,,,,0,,

logic:

instring=checked

&&

[SYSTEMS.MCP.MasterCaution]==[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=2,chklread,-1.000000,

execute=1,Autobrake?,0.000000,

logic:

instring=checked

&&

[SYSTEMS.MCP.MasterCaution]==[1.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Sir; master caution illuminate,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Descent checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Autobrake,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.BRAKES.AutoBrakeSW]<[2.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=1,Sir; autobrake is not set,0.000000,

execute=2,chklread,-1.000000,

execute=1,Landing data?,0.000000,

logic:

instring=any

&&

[SYSTEMS.BRAKES.AutoBrakeSW]>[1.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=0,#Set!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Landing data?,0.000000,

logic:

instring=say autobrake position

&&

[1.000000]==[0.000000]

calc=[0.000000]

logic:

calc=[0.000000]

out=LandingData,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.FMS.Vref]<[110.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=2,chcduinit,-1.000000,

execute=4,laminar/B738/button/fmc2_init_ref,0.000000,

execute=2,chcdul6,-1.000000,

execute=4,laminar/B738/button/fmc2_6L,0.000000,

execute=2,chcdul5,-1.000000,

execute=4,laminar/B738/button/fmc2_5L,0.000000,

execute=1,V reference is not set,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Descent checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

instring=any

&&

[SYSTEMS.FMS.MDA]<=[0.000000]

&&

[SYSTEMS.FMS.DH]==[0.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=1,Minimums is not set,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Descent checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

instring=say v reference speed and minimums

&&

[1.000000]==[0.000000]

calc=[0.000000]

logic:

instring=any

&&

[SYSTEMS.FMS.MDA]>[0.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

logic:

instring=any

&&

[SYSTEMS.FMS.DH]>[0.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

logic:

calc=[0.000000]

out=LandingData1,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=2,chcduinit,-1.000000,

execute=4,laminar/B738/button/fmc2_init_ref,0.000000,

execute=2,chcdul6,-1.000000,

execute=4,laminar/B738/button/fmc2_6L,0.000000,

execute=2,chcdul5,-1.000000,

execute=4,laminar/B738/button/fmc2_5L,0.000000,

execute=1,V reference <SYSTEMS.FMS.Vref>,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=LandingData2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MCP.RadioSwCap]==[0.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chklminsdn,-1.000000,

execute=8,jd/fo/needsetdh,0.000000,

execute=8,laminar/B738/EFIS_control/fo/minimums_show,1.000000,

execute=8,laminar/B738/EFIS_control/fo/minimums,0.000000,

execute=2,chklminsup,-1.000000,

execute=8,jd/fo/needsetdh,1.000000,

execute=7,,1.000000,

execute=1,Minimums <SYSTEMS.MCP.DH_CoPilot> set,0.000000,

execute=2,chklread,-1.000000,

execute=0,Approach briefing?,0.000000,

logic:

[SYSTEMS.MCP.RadioSwCap]==[1.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chklminsdn,-1.000000,

execute=8,jd/fo/needsetmda,0.000000,

execute=8,laminar/B738/EFIS_control/fo/minimums_show,1.000000,

execute=8,laminar/B738/EFIS_control/fo/minimums,1.000000,

execute=2,chklminsup,-1.000000,

execute=8,jd/fo/needsetmda,1.000000,

execute=7,,1.000000,

execute=1,Minimums baro <SYSTEMS.MCP.MDA_CoPilot> set,0.000000,

execute=2,chklread,-1.000000,

execute=0,Approach briefing?,0.000000,

logic:

calc=[0.000000]

out=ApprBrief,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=0,#Complete!,0.000000,

logic:

[0.000000]==[1.000000]

&&

instring=complete

calc=[0.000000]

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[1.000000]

execute=2,chklread,-1.000000,

execute=12,descent checklist,-1.000000,

execute=8,jd/fo/needsetdh,0.000000,

execute=8,jd/fo/needsetdh,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Descent checklist complete,0.000000,

logic:

calc=[0.000000]



devstack=Approach

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=approach checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,approach checklist,-1.000000,

execute=1,Approach checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Altimeters?,0.000000,

logic:

instring=approach checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed on the ground!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Altim,integer,,0.000000,,,,,,,,0,,

logic:

instring=say baro pressure on the pfd

&&

[1.000000]==[0.000000]

calc=[0.000000]

logic:

instring=any

&&

[SYSTEMS.MCP.BaroStdCap]==[1.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chkl-mcp,-1.000000,

execute=1,Sir; you have a standard baro set,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Approach checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

instring=any

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

logic:

calc=[0.000000]

out=Altim1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MCP.ChangeHPA_Cap]==[0.000000]

&&

[SYSTEMS.MCP.ChangeHPA_Fo]==[0.000000]

&&

[SYSTEMS.MCP.BaroStdFo]==[0.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chklbarodn,-1.000000,

execute=8,jd/fo/needsetbaro1,0.000000,

execute=8,jd/fo/needsetbaro1,1.000000,

execute=2,chklbaroup,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=1,QNH <&SYSTEMS.MCP.BaroSetInHgFo100> set,0.000000,

execute=1,Altitude passing <SYSTEMS.POSITION.AltimFO> now,0.000000,

logic:

[SYSTEMS.MCP.ChangeHPA_Cap]==[0.000000]

&&

[SYSTEMS.MCP.ChangeHPA_Fo]==[1.000000]

&&

[SYSTEMS.MCP.BaroStdFo]==[0.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chklbarodn,-1.000000,

execute=4,laminar/B738/EFIS_control/fo/baro_in_hpa_dn,0.000000,

execute=8,jd/fo/needsetbaro1,0.000000,

execute=8,jd/fo/needsetbaro1,1.000000,

execute=2,chklbaroup,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=1,QNH <&SYSTEMS.MCP.BaroSetInHgFo100> set,0.000000,

execute=1,Altitude passing <SYSTEMS.POSITION.AltimFO> now,0.000000,

logic:

[SYSTEMS.MCP.ChangeHPA_Cap]==[0.000000]

&&

[SYSTEMS.MCP.ChangeHPA_Fo]==[0.000000]

&&

[SYSTEMS.MCP.BaroStdFo]==[1.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chklbarodn,-1.000000,

execute=4,laminar/B738/EFIS_control/fo/push_button/std_press,0.000000,

execute=8,jd/fo/needsetbaro1,0.000000,

execute=8,jd/fo/needsetbaro1,1.000000,

execute=2,chklbaroup,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=1,QNH <&SYSTEMS.MCP.BaroSetInHgFo100> set,0.000000,

execute=1,Altitude passing <SYSTEMS.POSITION.AltimFO> now,0.000000,

logic:

[SYSTEMS.MCP.ChangeHPA_Cap]==[0.000000]

&&

[SYSTEMS.MCP.ChangeHPA_Fo]==[1.000000]

&&

[SYSTEMS.MCP.BaroStdFo]==[1.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chklbarodn,-1.000000,

execute=4,laminar/B738/EFIS_control/fo/baro_in_hpa_dn,0.000000,

execute=4,laminar/B738/EFIS_control/fo/push_button/std_press,0.000000,

execute=8,jd/fo/needsetbaro1,0.000000,

execute=8,jd/fo/needsetbaro1,1.000000,

execute=2,chklbaroup,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=1,QNH <&SYSTEMS.MCP.BaroSetInHgFo100> set,0.000000,

execute=1,Altitude passing <SYSTEMS.POSITION.AltimFO> now,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Altim3,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.MCP.ChangeHPA_Cap]==[1.000000]

&&

[SYSTEMS.MCP.ChangeHPA_Fo]==[1.000000]

&&

[SYSTEMS.MCP.BaroStdFo]==[0.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chklbarodn,-1.000000,

execute=8,jd/fo/needsetbaro1,0.000000,

execute=8,jd/fo/needsetbaro1,1.000000,

execute=2,chklbaroup,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=1,QNH <&SYSTEMS.MCP.BaroSetHpaFO> set,0.000000,

execute=1,Altitude passing <SYSTEMS.POSITION.AltimFO> now,0.000000,

logic:

[SYSTEMS.MCP.ChangeHPA_Cap]==[1.000000]

&&

[SYSTEMS.MCP.ChangeHPA_Fo]==[0.000000]

&&

[SYSTEMS.MCP.BaroStdFo]==[0.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chklbarodn,-1.000000,

execute=4,laminar/B738/EFIS_control/fo/baro_in_hpa_up,0.000000,

execute=8,jd/fo/needsetbaro1,0.000000,

execute=8,jd/fo/needsetbaro1,1.000000,

execute=2,chklbaroup,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=1,QNH <&SYSTEMS.MCP.BaroSetHpaFO> set,0.000000,

execute=1,Altitude passing <SYSTEMS.POSITION.AltimFO> now,0.000000,

logic:

[SYSTEMS.MCP.ChangeHPA_Cap]==[1.000000]

&&

[SYSTEMS.MCP.ChangeHPA_Fo]==[1.000000]

&&

[SYSTEMS.MCP.BaroStdFo]==[1.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chklbarodn,-1.000000,

execute=4,laminar/B738/EFIS_control/fo/push_button/std_press,0.000000,

execute=8,jd/fo/needsetbaro1,0.000000,

execute=8,jd/fo/needsetbaro1,1.000000,

execute=2,chklbaroup,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=1,QNH <&SYSTEMS.MCP.BaroSetHpaFO> set,0.000000,

execute=1,Altitude passing <SYSTEMS.POSITION.AltimFO> now,0.000000,

logic:

[SYSTEMS.MCP.ChangeHPA_Cap]==[1.000000]

&&

[SYSTEMS.MCP.ChangeHPA_Fo]==[0.000000]

&&

[SYSTEMS.MCP.BaroStdFo]==[1.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chklbarodn,-1.000000,

execute=4,laminar/B738/EFIS_control/fo/baro_in_hpa_up,0.000000,

execute=4,laminar/B738/EFIS_control/fo/push_button/std_press,0.000000,

execute=8,jd/fo/needsetbaro1,0.000000,

execute=8,jd/fo/needsetbaro1,1.000000,

execute=2,chklbaroup,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=1,QNH <&SYSTEMS.MCP.BaroSetHpaFO> set,0.000000,

execute=1,Altitude passing <SYSTEMS.POSITION.AltimFO> now,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[1.000000]

execute=2,chklread,-1.000000,

execute=12,approach checklist,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Approach checklist complete,0.000000,

logic:

calc=[0.000000]



devstack=Landing

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=landing checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,landing checklist,-1.000000,

execute=1,Landing checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklovhddn,-1.000000,

execute=1,Engine start switches?,0.000000,

logic:

instring=landing checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed on the ground!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=EngStart,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.ENGINE.Eng1StartSW]==[2.000000]

&&

[SYSTEMS.ENGINE.Eng2StartSW]==[2.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

logic:

instring=continuous

&&

[1.000000]==[0.000000]

calc=[0.000000]

logic:

[SYSTEMS.ENGINE.Eng2StartSW]!=[2.000000]

||

[SYSTEMS.ENGINE.Eng1StartSW]!=[2.000000]

&&

instring=any

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=1,Are not set in continuous position,0.000000,

execute=0,I just set,0.000000,

logic:

calc=[0.000000]

out=Eng1StartSW,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng1StartSW]!=[2.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,start1auto,-1.000000,

execute=4,laminar/B738/knob/eng1_start_right,0.000000,

execute=2,start1cont,0.000000,

execute=2,ovhd-dn,-1.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Eng2StartSW,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng2StartSW]!=[2.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,start2auto,-1.000000,

execute=4,laminar/B738/knob/eng2_start_right,0.000000,

execute=2,start2cont,0.000000,

execute=2,ovhd-dn,-1.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=EngStartSW,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ENGINE.Eng1StartSW]==[2.000000]

&&

[SYSTEMS.ENGINE.Eng2StartSW]==[2.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=0,#Continuous!,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklread,-1.000000,

execute=1,Speed brake?,0.000000,

logic:

calc=[0.000000]

out=SpeedBrake,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.SPEEDBRAKE.SB_DrfSim]==[-0.500000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=0,#Armed!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Landing gear?,0.000000,

logic:

instring=any

&&

[SYSTEMS.SPEEDBRAKE.SB_DrfSim]!=[-0.500000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=1,Speed brake is not arm,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Landing checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

instring=arm

&&

[1.000000]==[0.000000]

calc=[0.000000]

logic:

calc=[0.000000]

out=LandingGear,integer,,0.000000,,,,,,,,0,,

logic:

instring=down

&&

[SYSTEMS.LG.LG_Lever]!=[1.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=1,Sir; gear is not down,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Landing checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

instring=down

&&

[SYSTEMS.LG.LG_Lever]==[1.000000]

calc=[0.000000]

execute=2,chkl-cdu,-1.000000,

execute=0,#Down!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Flaps?,0.000000,

logic:

calc=[0.000000]

out=Flaps,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.FLAPS.FlapsMove]==[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-ped,-1.000000,

execute=1,Flaps is not set,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Landing checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

instring=any

&&

[SYSTEMS.FLAPS.FlapCompApp]!=[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-ped,-1.000000,

execute=1,Flaps are not set for landing position,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Landing checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

instring=any

&&

[SYSTEMS.FLAPS.FlapCompApp]==[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=0,#Set for landing!,0.000000,

execute=2,chkl-ped,-1.000000,

logic:

instring=say flap position

&&

[0.000000]==[1.000000]

calc=[0.000000]

logic:

instring=any

&&

[SYSTEMS.FMS.FlapsAppr]<[0.625000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-ped,-1.000000,

execute=1,This position of the flaps is not used for landing,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Landing checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[1.000000]

execute=2,chklread,-1.000000,

execute=12,landing checklist,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Landing checklist complete,0.000000,

logic:

calc=[0.000000]



devstack=Shutdown

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=shutdown checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,shutdown checklist,-1.000000,

execute=1,Shutdown checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklovhddn,-1.000000,

execute=1,Fuel pumps?,0.000000,

logic:

instring=shutdown checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed in flight!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Pump1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LAftPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,ovhd-dn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,aft-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft1,0.000000,

execute=2,aft-l-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pump2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]!=[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[0.000000]

calc=[0.000000]

execute=2,ovhd-dn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,fwd-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft2,0.000000,

execute=2,fwd-l-off,0.000000,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]==[1.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]<[200.000000]

calc=[0.000000]

execute=10,not_define,0.000000,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]==[1.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]>[200.000000]

calc=[0.000000]

execute=2,ovhd-dn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,fwd-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft2,0.000000,

execute=2,fwd-l-off,0.000000,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]==[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]<[200.000000]

calc=[0.000000]

execute=2,ovhd-dn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,fwd-l-off,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft2,1.000000,

execute=2,fwd-l-on,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pump3,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RFwdPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,ovhd-dn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,fwd-r-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_rgt2,0.000000,

execute=2,fwd-r-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pump4,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RAftPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,ovhd-dn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,aft-r-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_rgt1,0.000000,

execute=2,aft-r-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pump5,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LCtrPumpSW]!=[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[0.000000]

calc=[0.000000]

execute=2,ovhd-dn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,ctr-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr1,0.000000,

execute=2,ctr-l-off,0.000000,

logic:

[SYSTEMS.FUEL.LCtrPumpSW]==[1.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]>[200.000000]

calc=[0.000000]

execute=10,not_define,0.000000,

logic:

[SYSTEMS.FUEL.LCtrPumpSW]==[1.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]<[200.000000]

calc=[0.000000]

execute=2,ovhd-dn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,ctr-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr1,0.000000,

execute=2,ctr-l-off,0.000000,

logic:

[SYSTEMS.FUEL.LCtrPumpSW]==[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.FUEL.CenterTank]>[200.000000]

calc=[0.000000]

execute=2,ovhd-dn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,ctr-l-off,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr1,1.000000,

execute=2,ctr-l-on,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pump6,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RCtrPumpSW]!=[0.000000]

calc=[0.000000]

execute=2,ovhd-dn,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,ctr-r-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr2,0.000000,

execute=2,ctr-r-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=FuelPumps,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.PumpsAll]==[1.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Probe heat?,0.000000,

logic:

[SYSTEMS.FUEL.PumpsAll]!=[1.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,As required,0.000000,

execute=2,chklread,-1.000000,

execute=1,Probe heat?,0.000000,

logic:

calc=[0.000000]

out=ProbeHeatA,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ProbeHeatA]==[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,probeaon,-1.000000,

execute=8,laminar/B738/toggle_switch/capt_probes_pos,0.000000,

execute=2,probeaoff,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=ProbeHeatB,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ProbeHeatB]==[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,probebon,-1.000000,

execute=8,laminar/B738/toggle_switch/fo_probes_pos,0.000000,

execute=2,probeboff,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=ProbeHeat,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ICE.ProbeHeatA]==[0.000000]

&&

[SYSTEMS.ICE.ProbeHeatB]==[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Hydraulic panel?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

calc=[0.000000]

out=HydEng1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.Eng1PumpSW]!=[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,hydeng1off,-1.000000,

execute=8,laminar/B738/toggle_switch/hydro_pumps1_pos,1.000000,

execute=2,hydeng1on,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=HydEng2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.Eng2PumpSW]!=[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,hydeng2off,-1.000000,

execute=8,laminar/B738/toggle_switch/hydro_pumps2_pos,1.000000,

execute=2,hydeng2on,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=HydElec1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.ElecPump1]!=[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,helec1on,-1.000000,

execute=8,laminar/B738/toggle_switch/electric_hydro_pumps2_pos,0.000000,

execute=2,helec1off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=HydElec2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.ElecPump2]!=[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,helec2on,-1.000000,

execute=8,laminar/B738/toggle_switch/electric_hydro_pumps1_pos,0.000000,

execute=2,helec2off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=HydSet,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.HYD.Eng1PumpSW]==[1.000000]

&&

[SYSTEMS.HYD.Eng2PumpSW]==[1.000000]

&&

[SYSTEMS.HYD.ElecPump2]==[0.000000]

&&

[SYSTEMS.HYD.ElecPump2]==[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Set,0.000000,

execute=2,chklread,-1.000000,

execute=1,Flaps?,0.000000,

logic:

calc=[0.000000]

out=Flaps,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FLAPS.FlapsMove]>[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-ped,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,flaps,-1.000000,

execute=8,laminar/B738/flt_ctrls/flap_lever,0.000000,

execute=2,flaps0,0.000000,

execute=1,Up,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklread,-1.000000,

execute=1,Parking brake?,0.000000,

logic:

[SYSTEMS.FLAPS.FlapsMove]==[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-ped,-1.000000,

execute=1,Up,0.000000,

execute=2,chklread,-1.000000,

execute=1,Parking brake?,0.000000,

logic:

calc=[0.000000]

out=ParkingBrake,integer,,0.000000,,,,,,,,0,,

logic:

instring=set

&&

[SYSTEMS.BRAKES.ParkBrakeHandlePos]==[1.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=0,#Set!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Engine start levers?,0.000000,

logic:

instring=set

&&

[SYSTEMS.BRAKES.ParkBrakeHandlePos]==[0.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=7,,0.300000,

execute=1,Parking brake is not set,0.000000,

execute=2,chklread,-1.000000,

execute=1,Engine start levers?,0.000000,

logic:

calc=[0.000000]

out=EngStartLever,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.ENGINE.EngMastSumm]==[0.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=7,,0.300000,

execute=0,#Cut off!,0.000000,

execute=2,chklread,-1.000000,

execute=1,Weather radar?,0.000000,

logic:

instring=any

&&

[SYSTEMS.ENGINE.EngMastSumm]>[0.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=1,Engine start levers is not cutoff,0.000000,

execute=1,Shutdown checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

instring=cutoff

&&

[0.000000]==[1.000000]

calc=[0.000000]

logic:

calc=[0.000000]

out=WeatherRadar,integer,,0.000000,,,,,,,,0,,

logic:

instring=off

&&

[SYSTEMS.PEDESTAL.RadarSWCap]==[1.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=1,Your weather radar is not off,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,Shutdown checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

instring=off

&&

[SYSTEMS.PEDESTAL.RadarSWFo]==[1.000000]

calc=[0.000000]

execute=2,chkl-frd,-1.000000,

execute=2,chklwxr,-1.000000,

execute=4,laminar/B738/EFIS_control/fo/push_button/wxr_press,0.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,IRS mode selectors?,0.000000,

logic:

instring=any

&&

[SYSTEMS.PEDESTAL.RadarSWCap]==[0.000000]

&&

[SYSTEMS.PEDESTAL.RadarSWFo]==[0.000000]

calc=[0.000000]

execute=2,chkl-mcp,-1.000000,

execute=2,chkl-frd,-1.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,IRS mode selectors?,0.000000,

logic:

calc=[0.000000]

out=IRS1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDUP.IRS_L]!=[0.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,irs-l-nav,-1.000000,

execute=4,laminar/B738/toggle_switch/irs_L_left,0.000000,

execute=4,laminar/B738/toggle_switch/irs_L_left,0.000000,

execute=4,laminar/B738/toggle_switch/irs_L_left,0.000000,

execute=2,irs-l-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=IRS2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDUP.IRS_R]!=[0.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,irs-r-nav,-1.000000,

execute=4,laminar/B738/toggle_switch/irs_R_left,0.000000,

execute=4,laminar/B738/toggle_switch/irs_R_left,0.000000,

execute=4,laminar/B738/toggle_switch/irs_R_left,0.000000,

execute=2,irs-r-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=IRS,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDUP.IRS_L]==[0.000000]

&&

[SYSTEMS.OVHDUP.IRS_R]==[0.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Off,0.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[1.000000]

execute=2,chklread,-1.000000,

execute=12,shutdown checklist,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Shutdown checklist complete,0.000000,

logic:

calc=[0.000000]



devstack=Secure

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=secure checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,secure checklist,-1.000000,

execute=1,Secure checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklovhddn,-1.000000,

execute=1,Fuel pumps?,0.000000,

logic:

instring=secure checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed in flight!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Pump1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LAftPumpSW]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,aft-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft1,0.000000,

execute=2,aft-l-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pump2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LFwdPumpSW]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,fwd-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_lft2,0.000000,

execute=2,fwd-l-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pump3,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RFwdPumpSW]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,fwd-r-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_rgt2,0.000000,

execute=2,fwd-r-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pump4,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RAftPumpSW]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,aft-r-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_rgt1,0.000000,

execute=2,aft-r-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pump5,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.LCtrPumpSW]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,ctr-l-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr1,0.000000,

execute=2,ctr-l-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pump6,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.RCtrPumpSW]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,ctr-r-on,-1.000000,

execute=8,laminar/B738/fuel/fuel_tank_pos_ctr2,0.000000,

execute=2,ctr-r-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=FuelPumps,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FUEL.PumpsAll]==[0.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Pumps off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Emergency exit lights?,0.000000,

logic:

calc=[0.000000]

out=EmerExit,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.EmerExitSW]!=[0.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,exiton,-1.000000,

execute=4,laminar/B738/push_button/emer_exit_full_off,0.000000,

execute=2,exitoff,0.000000,

execute=1,Off,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklread,-1.000000,

execute=1,Window heat?,0.000000,

logic:

[SYSTEMS.LIGHTS.EmerExitSW]==[0.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Window heat?,0.000000,

logic:

calc=[0.000000]

out=WindowHeat1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WHeatLSide]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,wh1-on,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_l_side,0.000000,

execute=2,wh1-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=WindowHeat2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WHeatLFwd]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,wh2-on,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_l_fwd,0.000000,

execute=2,wh2-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=WindowHeat3,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WHeatRFwd]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,wh3-on,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_r_fwd,0.000000,

execute=2,wh3-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=WindowHeat4,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.OVHDSIDEL.WHeatRSide]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,wh4-on,-1.000000,

execute=4,laminar/B738/toggle_switch/window_heat_r_side,0.000000,

execute=2,wh4-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=WindowHeat,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Packs?,0.000000,

logic:

calc=[0.000000]

out=Pack1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Pack1]==[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,pack-1-aut,-1.000000,

execute=8,laminar/B738/air/l_pack_pos,0.000000,

execute=2,pack-1-off,0.000000,

logic:

[SYSTEMS.AIR.Pack1]==[2.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,pack-1-hig,-1.000000,

execute=8,laminar/B738/air/l_pack_pos,0.000000,

execute=2,pack-1-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Pack2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Pack2]==[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,pack-2-aut,-1.000000,

execute=8,laminar/B738/air/r_pack_pos,0.000000,

execute=2,pack-2-off,0.000000,

logic:

[SYSTEMS.AIR.Pack2]==[2.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,pack-2-hig,-1.000000,

execute=8,laminar/B738/air/r_pack_pos,0.000000,

execute=2,pack-2-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Packs,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Pack1]==[0.000000]

&&

[SYSTEMS.AIR.Pack2]==[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,APU bleed?,0.000000,

logic:

calc=[0.000000]

out=ApuBleed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.APUBleedSW]==[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,apubleedon,-1.000000,

execute=8,laminar/B738/toggle_switch/bleed_air_apu_pos,0.000000,

execute=2,apuble-off,0.000000,

execute=1,Off,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklread,-1.000000,

execute=1,Lights?,0.000000,

logic:

[SYSTEMS.AIR.APUBleedSW]==[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Lights?,0.000000,

logic:

calc=[0.000000]

out=Lights1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_LandLSW]!=[0.000000]

||

[SYSTEMS.LIGHTS.OVHD_LandRSW]!=[0.000000]

||

[SYSTEMS.LIGHTS.OVHD_LandLRetr]!=[0.000000]

||

[SYSTEMS.LIGHTS.OVHD_LandRRetr]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,all-1-on,-1.000000,

execute=4,laminar/B738/switch/land_lights_ret_right_up,0.000000,

execute=4,laminar/B738/switch/land_lights_ret_right_up,0.000000,

execute=4,laminar/B738/switch/land_lights_ret_left_up,0.000000,

execute=4,laminar/B738/switch/land_lights_ret_left_up,0.000000,

execute=8,laminar/B738/switch/land_lights_left_pos,0.000000,

execute=8,laminar/B738/switch/land_lights_right_pos,0.000000,

execute=2,all-1-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Lights2,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_RwyLeftSW]==[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,runwayonl,-1.000000,

execute=4,laminar/B738/switch/rwy_light_left_off,0.000000,

execute=2,runwayoffl,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Lights3,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_RwyRightSW]==[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,runwayonr,-1.000000,

execute=4,laminar/B738/switch/rwy_light_right_off,0.000000,

execute=2,runwayoffr,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Lights4,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_TaxiSW]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,taxi-on,-1.000000,

execute=4,laminar/B738/toggle_switch/taxi_light_brightness_pos_up,0.000000,

execute=4,laminar/B738/toggle_switch/taxi_light_brightness_pos_up,0.000000,

execute=2,taxi-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Lights5,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_LogoSW]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,logo-on,-1.000000,

execute=8,laminar/B738/toggle_switch/logo_light,0.000000,

execute=2,logo-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Lights6,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_NavSW]==[-1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,strobe-nav,-1.000000,

execute=4,laminar/B738/toggle_switch/position_light_up,0.000000,

execute=2,strobe-off,0.000000,

logic:

[SYSTEMS.LIGHTS.OVHD_NavSW]==[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,strobe-on,-1.000000,

execute=4,laminar/B738/toggle_switch/position_light_down,0.000000,

execute=2,strobe-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Lights7,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_BeaconSW]!=[0.000000]

calc=[0.000000]

execute=2,beacon-on,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=8,sim/cockpit/electrical/beacon_lights_on,0.000000,

execute=2,beacon-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Lights8,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_WingSW]!=[0.000000]

calc=[0.000000]

execute=2,wing-on,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=4,laminar/B738/switch/wing_light_off,0.000000,

execute=2,wing-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Lights9,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.LIGHTS.OVHD_WheelSW]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,well-on,-1.000000,

execute=8,sim/cockpit2/switches/generic_lights_switch[5],0.000000,

execute=2,well-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Lights,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,APU?,0.000000,

logic:

calc=[0.000000]

out=APU,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.APU.StartSW]>[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,apu-start,-1.000000,

execute=4,laminar/B738/spring_toggle_switch/APU_start_pos_up,0.000000,

execute=4,laminar/B738/spring_toggle_switch/APU_start_pos_up,0.000000,

execute=2,apu-off,0.000000,

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Battery switch?,0.000000,

logic:

[SYSTEMS.APU.StartSW]==[1.000000]

&&

[SYSTEMS.APU.AvailAPU]==[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,apu-start,-1.000000,

execute=4,laminar/B738/spring_toggle_switch/APU_start_pos_up,0.000000,

execute=4,laminar/B738/spring_toggle_switch/APU_start_pos_up,0.000000,

execute=2,apu-off,0.000000,

execute=2,chklovhddn,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Battery switch?,0.000000,

logic:

[SYSTEMS.APU.StartSW]==[0.000000]

&&

[SYSTEMS.APU.AvailAPU]==[0.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Battery switch?,0.000000,

logic:

calc=[0.000000]

out=Battery,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.ELEC.BatterySW]!=[0.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,batton,-1.000000,

execute=4,laminar/B738/button_switch_cover02,0.000000,

execute=7,,0.200000,

execute=8,laminar/B738/electric/battery_pos,0.000000,

execute=2,battoff,0.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

logic:

[SYSTEMS.ELEC.BatterySW]==[0.000000]

calc=[0.000000]

execute=2,chklovhdup,-1.000000,

execute=1,Off,0.000000,

execute=2,chklread,-1.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[1.000000]

execute=2,chklread,-1.000000,

execute=12,secure checklist,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Secure checklist complete,0.000000,

logic:

calc=[0.000000]



devstack=Before de icing

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=before de icing checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=12,Expected Answer,5.000000,

execute=1,Before de icing checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,A P U?,0.000000,

execute=2,chklovhddn,-1.000000,

logic:

instring=before de icing checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed in flight!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Apu,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.APU.AvailAPU]==[0.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=0,Is off,0.000000,

execute=2,chklread,-1.000000,

execute=0,Flaps?,0.000000,

execute=2,chkl-ped,-1.000000,

logic:

[SYSTEMS.APU.AvailAPU]==[1.000000]

calc=[0.000000]

execute=2,chklovhddn,-1.000000,

execute=0,Is on,0.000000,

execute=2,chklread,-1.000000,

execute=0,Flaps?,0.000000,

execute=2,chkl-ped,-1.000000,

logic:

calc=[0.000000]

out=Flaps,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.FLAPS.FlapLever]!=[0.000000]

&&

[SYSTEMS.FLAPS.Ok0]==[1.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,flaps,-1.000000,

execute=8,laminar/B738/flt_ctrls/flap_lever,0.000000,

execute=2,flaps0,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=0,Retracted,0.000000,

execute=2,chklread,-1.000000,

execute=1,Thrust levers?,0.000000,

execute=2,chkl-ped,-1.000000,

execute=2,chklanswer,-1.000000,

logic:

[SYSTEMS.FLAPS.FlapLever]==[0.000000]

&&

[SYSTEMS.FLAPS.Ok0]==[1.000000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=0,Checked; Up set,0.000000,

execute=2,chklread,-1.000000,

execute=1,Thrust levers?,0.000000,

execute=2,chkl-ped,-1.000000,

logic:

calc=[0.000000]

out=ThrusLever,integer,,0.000000,,,,,,,,0,,

logic:

instring=idle

&&

[SYSTEMS.ENGINE.Eng1Lever]<[0.200000]

&&

[SYSTEMS.ENGINE.Eng2Lever]<[0.200000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chklread,-1.000000,

execute=1,Stabilizer trim?,0.000000,

execute=2,chkl-ped,-1.000000,

logic:

instring=idle

&&

[SYSTEMS.ENGINE.Eng1Lever]>[0.200000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=0,Sir; is not idle position,0.000000,

execute=2,chklanswer,-1.000000,

execute=0,Before de icing checklist is not complete,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=3,,0.000000,

logic:

instring=idle

&&

[SYSTEMS.ENGINE.Eng2Lever]>[0.200000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=0,Sir; is not idle position,0.000000,

execute=2,chklanswer,-1.000000,

execute=0,Before de icing checklist is not complete,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Trim,integer,,0.000000,,,,,,,,0,,

logic:

instring=any

&&

[SYSTEMS.THS.ThsError]<[0.250000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=2,chklread,-1.000000,

execute=1,Engine bleed air switches?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

instring=any

&&

[SYSTEMS.THS.ThsError]>[0.250000]

calc=[0.000000]

execute=2,chkl-ped,-1.000000,

execute=1,Is not set in takeoff position,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=0,Before de icing checklist is not complete,0.000000,

execute=3,,0.000000,

logic:

[0.000000]==[1.000000]

&&

instring=check and set trim for takeoff position

calc=[0.000000]

logic:

calc=[0.000000]

out=Eng1Bleed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Eng1BleedSW]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,bleed1-on,-1.000000,

execute=8,laminar/B738/toggle_switch/bleed_air_1_pos,0.000000,

execute=2,bleed1-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Eng2Bleed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Eng2BleedSW]!=[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,bleed2-on,-1.000000,

execute=8,laminar/B738/toggle_switch/bleed_air_2_pos,0.000000,

execute=2,bleed2-off,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=EngineBleed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Eng1BleedSW]==[0.000000]

&&

[SYSTEMS.AIR.Eng2BleedSW]==[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Is off,0.000000,

execute=2,chklread,-1.000000,

execute=1,A P U bleed air switch?,0.000000,

logic:

calc=[0.000000]

out=APUBleed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.APUBleedSW]==[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,apubleedon,-1.000000,

execute=8,laminar/B738/toggle_switch/bleed_air_apu_pos,0.000000,

execute=2,apuble-off,0.000000,

execute=1,Is off,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklread,-1.000000,

logic:

[SYSTEMS.AIR.APUBleedSW]==[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=1,Is off,0.000000,

execute=2,chklread,-1.000000,

logic:

calc=[0.000000]

out=End,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=1,Before de icing checklist!,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,Before de icing checklist complete,0.000000,

logic:

calc=[0.000000]



devstack=After de icing

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

instring=after de icing checklist

&&

[SYSTEMS.POSITION.onAir]==[0.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=1,After de icing checklist!,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Chrono?,0.000000,

execute=2,chkl-frd,-1.000000,

logic:

instring=after de icing checklist

&&

[SYSTEMS.POSITION.onAir]==[1.000000]

calc=[0.000000]

execute=2,answer01,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=1,This checklist cannot be performed in flight!,0.000000,

execute=3,,0.000000,

logic:

calc=[0.000000]

out=Chrono,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.TIME.Chrono]==[-1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,chrono,-1.000000,

execute=4,laminar/B738/push_button/chrono_cycle_fo,0.000000,

execute=0,Wait one minute,0.000000,

execute=2,look-frd,-1.000000,

logic:

[SYSTEMS.TIME.Chrono]==[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,chrono,-1.000000,

execute=4,laminar/B738/push_button/chrono_cycle_fo,0.000000,

execute=4,laminar/B738/push_button/chrono_cycle_fo,0.000000,

execute=4,laminar/B738/push_button/chrono_cycle_fo,0.000000,

execute=0,Wait one minute,0.000000,

execute=2,look-frd,-1.000000,

logic:

[SYSTEMS.TIME.Chrono]==[0.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,chrono,-1.000000,

execute=4,laminar/B738/push_button/chrono_cycle_fo,0.000000,

execute=4,laminar/B738/push_button/chrono_cycle_fo,0.000000,

execute=0,Wait one minute,0.000000,

execute=2,look-frd,-1.000000,

logic:

calc=[0.000000]

out=Chrono1,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.TIME.Timer1min]==[1.000000]

calc=[0.000000]

execute=2,chrono,-1.000000,

execute=4,laminar/B738/push_button/chrono_cycle_fo,0.000000,

execute=4,laminar/B738/push_button/chrono_cycle_fo,0.000000,

execute=2,chklread,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,A P U Bleed?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

calc=[0.000000]

out=APUBleed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.AIR.APUBleedSW]==[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=0,Is on,0.000000,

execute=2,chklread,-1.000000,

execute=1,Engine bleed air switches?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

[SYSTEMS.APU.AvailAPU]==[1.000000]

&&

[SYSTEMS.AIR.APUBleedSW]==[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,apuble-off,-1.000000,

execute=8,laminar/B738/toggle_switch/bleed_air_apu_pos,1.000000,

execute=2,apubleedon,0.000000,

execute=0,Is on,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklread,-1.000000,

execute=1,Engine bleed air switches?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

[SYSTEMS.APU.AvailAPU]==[0.000000]

&&

[SYSTEMS.AIR.APUBleedSW]==[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,apubleedon,-1.000000,

execute=8,laminar/B738/toggle_switch/bleed_air_apu_pos,0.000000,

execute=2,apuble-off,0.000000,

execute=0,Is off,0.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=2,chklread,-1.000000,

execute=1,Engine bleed air switches?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

[SYSTEMS.APU.AvailAPU]==[0.000000]

&&

[SYSTEMS.AIR.APUBleedSW]==[0.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=0,Is off,0.000000,

execute=2,chklread,-1.000000,

execute=1,Engine bleed air switches?,0.000000,

execute=2,chklovhdrt,-1.000000,

logic:

calc=[0.000000]

out=Eng1Bleed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Eng1BleedSW]!=[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,bleed1-off,-1.000000,

execute=8,laminar/B738/toggle_switch/bleed_air_1_pos,1.000000,

execute=2,bleed1-on,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=Eng2Bleed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Eng2BleedSW]!=[1.000000]

calc=[0.000000]

execute=8,jd/fo/_planshet,0.000000,

execute=2,bleed2-off,-1.000000,

execute=8,laminar/B738/toggle_switch/bleed_air_2_pos,1.000000,

execute=2,bleed2-on,0.000000,

logic:

calc=[0.000000]

execute=10,not_define,0.000000,

out=EngineBleed,integer,,0.000000,,,,,,,,0,,

logic:

[SYSTEMS.AIR.Eng1BleedSW]==[1.000000]

&&

[SYSTEMS.AIR.Eng2BleedSW]==[1.000000]

calc=[0.000000]

execute=2,chklovhdrt,-1.000000,

execute=8,jd/fo/_planshet,1.000000,

execute=1,Is on,0.000000,

execute=2,chklread,-1.000000,

logic:

calc=[0.000000]

out=Title,integer,,0.000000,,,,,,,,0,,

logic:

[0.000000]==[0.000000]

calc=[0.000000]

execute=2,chklread,-1.000000,

execute=1,After de icing checklist!,0.000000,

execute=8,jd/fo/_planshet,0.000000,

execute=2,answer01,-1.000000,

execute=1,After de icing checklist complete,0.000000,

logic:

calc=[0.000000]

